{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"merged":[[0,0,0,5]]}
["附件1:新建感觉统合室康复训练器材清单"]
["序号","名称","尺寸","技术参数","单位","数量"]
[1,"*多元秋千悬挂组合游戏架","长：4000mm \n宽：4000mm\n高：2400mm","整套器材包括承重量300公斤方通铁框连外包铁框保护软垫。(提供国家专业检测单位出具的承受拉力检测报告，承受重量不得低于300公斤）","套",1]
[2,"秋千升降\n吊绳套件","长：1500mm","承重量500公斤。10mm直径进口专业安全绳，不锈钢挂圈，进口专业升降器，2kn安全扣2个。4套（出具专业检测单位的承受重量检测报告）","套",2]
[3,"秋千旋转\n吊绳套件","长：1500mm","承重量500公斤。不锈钢旋转件，不锈钢挂圈，2kn安全扣2个。2套（出具专业检测单位的承受重量检测报告）","套",4]
[4,"T形木马秋千","长:1100mm\n宽:200mm\n高:1200mm","软垫秋千主体，2kn安全扣1个，活动触觉垫及滑轮拉绳。承重量160公斤。","套",1]
[5,"方形木马秋千","长：1200mm\n宽：200mm\n高：1500mm","软垫秋千主体，2kn安全扣2个，活动触觉垫及软垫扶手。承重量160公斤。","套",1]
[6,"方形平板秋千","长：700mm\n宽：700mm\n高：1500mm","软垫秋千主体，2kn安全扣2个，活动触觉垫。承重量135公斤。（提供专业检测机构出具的产品检测报告）","套",1]
[7,"内胎秋千","直径:900mm","秋千主体。承重量110公斤。","套",1]
[8,"飞碟秋千","直径：600mm\n高：1200mm","软垫秋千主体，2kn安全扣1个，活动触觉垫及滑轮拉绳。承重量140公斤。","套",1]
[9,"长方形平板秋千（带围边）","长：1200mm\n宽：600mm\n高：1500mm","软垫秋千主体，2kn安全扣2个，活动触觉垫。承重量136公斤。","套",1]
[10,"海棉保护垫","长：1500mm\n宽：1500mm\n高：200mm","外套为可更换棉布制作，内套防水尼龙布，埴充物料为海棉小方块。 - 2套","套",4]
[11,"*拉架浮弹床","长：2400mm\n宽：1200mm\n高：2400mm","整套器材包括承重量300公斤方通铁框连外包铁框保护软垫，彩色软垫屏障板，魔术黏贴游戏板，3套浮弹布。(提供国家专业检测单位出具的承受压力检测报告，承受压力不得低于300公斤）","套",1]
[12,"*攀岩组合器材套件（攀爬）","长：5000mm\n高：2400mm","整套器材包括承重量300公斤方通铁框连外包铁框保护软垫、彩色绳梯、木梯、彩色背板攀岩墙及软垫尼龙带织网。(提供国家专业检测单位出具的承受压力检测报告，承受压力不得低于300公斤）","套",1]
[13,"大龙球","65cm、75cm、85cm",null,"套",1]
[14,"花生球","90*40",null,"套",1]
[15,"陀螺椅","Φ90cm",null,"套",4]
[16,"*大型平衡组合软件","长：3000mm\n宽：300mm\n高：400mm","直角缝边制作。采用高弹性EVA制作内层，游戏者使用时海绵不会产生超过20mm的下陷，防水尼龙布作外层。（提供BS5852阻燃检测报告及EN71-3无毒检测报告）","套",1]
[17,"组合电子摇摆区",null,"利用墙壁三侧多感官声光互动，吸引幼儿进行与3协助游戏者时刻保持平衡，达到左右双侧协调身体动作训练功效。软垫外框内架，左右摇摆平台，灯光目标按键，大软槌，可调高低升降扶手摇摇板，弹力安全带一套，220v。目标区-1800W*2200H（mm) 摇摇板-1200L*600W*200H（mm）","套",1]
[18,"电子弹弹区","长：1000mm\n宽：1000mm\n高：1800mm","立体图案结构，弹跳板连软垫面，多个目标大按键连电子声音反应，220V。","套",1]
[19,"电子旋转区","长：1100mm\n宽：1100mm\n高：2200mm","立体果树结构，旋转板连软垫面，多个目标大按键连电子声音反应，220V。","套",1]
[20,"滑行平台","550 宽 X 2200mm长",null,"套",1]
[21,"大及小号滑行车（滑板）","大号 - 380宽 x 560长 x 150MM高     小号 - 380宽 x 560长 x 150MM高","承重量70公斤不变形，白色尼龙轮，50MM厚软垫表面，四侧防磨损尼龙边。每部滑行车配辅助活动配件　- 触觉垫1张，拉绳1条。每款1件。","套",2]
[22,"*双层组合地垫","100平方，50MM厚","外层BS5852阻燃标准布料，内层高弹性EVA粘贴海绵，每张地垫均附魔术贴拼贴，提供布料阻燃烧证书 。（提供国家地市级质量检测研究院出具的强制性认证报告）","平方",100]
[23,"*双人摇摆鸭","长：1170mm\n宽：300mm\n高：560mm","内层高弹性EVA组合，外层由不同颜色无毒阻燃防水尼龙布特制。（提供BS5852布料阻燃检测报告以及EN71-3无毒检测报告）","套",1]
[24,"*滚筒","外径:800mm \n内径：600mm","内层实木加高弹性EVA组合，外层由不同颜色无毒阻燃防水尼龙布特制。(提供BS5852海绵阻燃检测报告）","套",1]
[25,"*平面单色墙垫","宽：1000mm\n高：1200mm\n厚：65mm\n50平","直角缝边制作。防水尼龙布 - BS5852阻燃规格，EN71(第3部份)玩具安全无毒规格   高弹度海棉 - BS5852阻燃规格。（提供国家地市级质量检测研究院出具的强制性认证报告）","平米",50]
[26,"触觉训练墙","6400*1200mm","直角缝边制作。防水尼龙布 - BS5852阻燃规格，EN71(第3部份)玩具安全无毒规格   高弹度海棉 - BS5852阻燃规格，附安全证书。","平米",20]
[27,"地面防滑地毯",null,"绿色环保材料","平米",30]
[28,"万象组合",null,"根据使用方需求选定","套",1]
[29,"平衡板",null,"根据使用方需求选定","套",10]
[30,"独脚凳",null,"根据使用方需求选定","套",10]
[31,"压路机",null,"根据使用方需求选定","套",1]
[32,"旋转滑梯",null,"根据使用方需求选定","套",1]
[33,"滑行秋千",null,"根据使用方需求选定","套",1]
[34,"触觉训练套装",null,"根据使用方需求选定","套",3]
[35,"触觉探索区",null,"根据使用方需求选定","平方",5]
[36,"视听感知区",null,"根据使用方需求选定","平方",5]